	


How the Vapour Blasting works:
 
· The water/glass beads slurry is delivered via a pump to the hand-held nozzle

· Compressed air is added at the blast nozzle to accelerate the slurry on to the component surface 

· The water buffers and lubricates the particles on impact, allowing very fine finishes to be produced without damage to the component

· All oxidations and impurities are gently washed away, the result is easy to keep clean, smooth, satin sheen finish and the rest is history
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